IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
Time stamp: "2023-06-23T19:27:27"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Alternate UI 20.2.12.1"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1687537647 (2023-06-23T16:27:27Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "93631129 Washbasin faucet, 230/9 V, Bluetooth" | object type "93631129(2023):93631129 Washbasin faucet, 230/9 V, Bluetooth" | names: "93631129(2023):93631129 Washbasin faucet, 230/9 V, Bluetooth:12354" | material: "Brass" | property sets: Constraints, Dimensions, Identity Data, Mechanical, Other, Phasing

Types
  IFCVALVETYPE "93631129 Washbasin faucet, 230/9 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Constraints, Dimensions, Electrical, General, Green Building Properties, Identity Data

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0576809945730818 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00220434117315511 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalDepth = 167.912499519142 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 190.011550942724 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 68.9424017698872 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "4" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/93631129" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/93631129" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/93631129" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/93631129/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/93631129" (IFCTEXT)
    Group = "Washbasin faucet" (IFCTEXT)
    Keynote = "" (IFCTEXT)
    Long Marketing = "Electra 93 series give you a clean classic design with beautiful round body flowing into round spout design with a clear design line framing the faucet design. A Classic design with improved height for any installation. Key Features Aerator with Tilt function +/- 10° for more flexible installation Newest Sensor technology for better detection and operation comfort Bluetooth technology for easy adjustment to personalize settings Low Pressure Power Plug" (IFCTEXT)
    Manufacturer = "HANSA" (IFCTEXT)
    Market = "International;Germany;Austria;Switzerland;Belgium;Netherlands;Italy" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.hansa.com/93631129" (IFCTEXT)
    Model = "93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    Name_en = "93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "93631129" (IFCTEXT)
    Product Family = "HANSAELECTRA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/93631129" (IFCTEXT)
    Product URL = "http://static.hansa.com/93631129" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/93631129/en" (IFCTEXT)
    Type Comments = "" (IFCTEXT)
    Type Name = "93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.hansa.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "3S-installation system for safe and simple mounting" (IFCTEXT)
    Aerator = "Laminar stream" (IFCTEXT)
    Afterflow Period = "3 s (1-20 s)" (IFCTEXT)
    Automatic Flush Frequency = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Connection = "Flexible inlet pipes" (IFCTEXT)
    Connection Size = "G3/8" (IFCTEXT)
    Electronic Parts = ";Power supply;Light indicated function(s)" (IFCTEXT)
    Flow Rate At 300kPa With Flow Controller = 0.00282517333771909 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Temperature control handle" (IFCTEXT)
    Max Flow Period = "2 min (1 - 1800 s)" (IFCTEXT)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Mixing valve for manual temperature control;Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Mounting Holes = "1 hole" (IFCTEXT)
    Operating Distance = "20-130 mm (110/130/160 mm)" (IFCTEXT)
    Spout Projection = "124 mm" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature Adjustments = "Adjustable hot water stop (included, retrofittable)" (IFCTEXT)
    Working Pressure = "100 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "93631129(2023): 93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    Family and Type = "93631129(2023): 93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "93631129(2023): 93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    Type Id = "93631129(2023): 93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Level 1" (IFCLABEL)
    Family and Type = "Level: Level 1" (IFCLABEL)
    Type = "Level: Level 1" (IFCLABEL)
    Type Id = "Level: Level 1" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "HANSA" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "93631129(2023)" (IFCTEXT)
    Features = "Touchless;Plug transformer;Bluetooth®" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "93631129" (IFCTEXT)
    Name = "93631129 Washbasin faucet, 230/9 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "70x170x190 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Level 1" (IFCTEXT)
  Electrical | properties | on 1 type object
    Bluetooth = "5.x (D060576)" (IFCTEXT)
    Electrical Connection = "230 / 9 V" (IFCTEXT)
    Operating Voltage = 9. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
    Protection Class = "IP 55 / transformer IP 20" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "93631129(2023)" (IFCTEXT)
    ManufacturerName = "HANSA" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for wash basins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "01/06/2023" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "4057304019593" (IFCTEXT)
    EMC Directive = "2014/53/EU , 2011/65/EU" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
    ETIM Class Number = "EC010340 Electronic tap" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "568 x 182 x 78" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration Of Performance (DOP) = "http://static.hansa.com/doc/DoP" (IFCTEXT)
    URL Declaration of Asbestos = "http://static.hansa.com/doc/asbestos" (IFCTEXT)
    URL Declaration of Conformity = "http://static.hansa.com/DoC/93631129" (IFCTEXT)
    URL Declaration of SCIP = "http://static.hansa.com/doc/SCIP" (IFCTEXT)
    URL EU Packaging Declaration = "http://static.hansa.com/doc/packaging" (IFCTEXT)
    URL EcoLabel Declaration = "http://static.hansa.com/doc/EcoLabel" (IFCTEXT)
    URL REACH = "http://static.hansa.com/doc/reach" (IFCTEXT)
    URL UWL = "http://static.hansa.com/UWL/93631129" (IFCTEXT)
    URL WEEE = "http://static.hansa.com/WEEE/93631129" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)

Other addresses and roles
  2 x postal address (none given)