IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2020-07-14T18:10:24"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20190508_0315(x64) - Exporter 17.4.0.0 - Alternate UI 17.4.0.0"
Application: "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)"

People and organizations
  Person "vbu737AR" of Organization (no name given)
  Owner history of Person "vbu737AR" of Organization (no name given) | application "Autodesk Revit 2017 (ENU)" version "2017" identifier "Revit" by Organization "Autodesk Revit 2017 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "Boston", "MA"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "08866202 Washbasin faucet, 6 V, Bluetooth" | object type "08866202 Washbasin faucet, 6 V, Bluetooth" | names: "08866202(2020):08866202 Washbasin faucet, 6 V, Bluetooth:371059" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "08866202 Washbasin faucet, 6 V, Bluetooth" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions(Type), Electrical Engineering(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Hansa" (IFCTEXT)
    Category = "Health & Care" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "08866202(2020)" (IFCTEXT)
    Features = "Thermostatic;Touchless;Bluetooth®;Battery-operated" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "08866202" (IFCTEXT)
    Name = "08866202 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "275x200x300 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.hansa.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.hansa.com/bim/08866202" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.hansa.com/catdrw/08866202" (IFCTEXT)
    Class = "Thermostatic;Touchless;Bluetooth®;Battery-operated" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.hansa.com/dimdrw/08866202" (IFCTEXT)
    FDV Document URL = "http://www.hansa.com/datasheet/08866202/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.hansa.com/flowchart/08866202" (IFCTEXT)
    Group = "Washbasin faucets" (IFCTEXT)
    Manufacturer = "Hansa" (IFCTEXT)
    Market = "INT;DEU;AUT;CHE;BEL;NLD;FRA;CZE;ITA;ESP;GRC;PRT" (IFCTEXT)
    Model = "08866202 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    Name_en = "08866202 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Package Weight = "2.84 kg" (IFCTEXT)
    Package external Dimensions = "295 x 180 x 115" (IFCTEXT)
    Product Code = "08866202" (IFCTEXT)
    Product Datasheet = "http://www.hansa.com/datasheet/08866202/en" (IFCTEXT)
    Product Family = "HANSACLINICA" (IFCTEXT)
    Product Image URL = "http://static.hansa.com/image/08866202" (IFCTEXT)
    Product URL = "http://static.hansa.com/08866202" (IFCTEXT)
    Product data url = "1" (IFCTEXT)
    Technical DataSheet URL = "http://www.hansa.com/datasheet/08866202/en" (IFCTEXT)
    Type Name = "08866202 Washbasin faucet, 6 V, Bluetooth" (IFCTEXT)
    URL = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Hansa" (IFCLABEL)
    ModelReference = "08866202" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "08866202 Washbasin faucet, 6 V, Bluetooth" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.173466898484452 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    InletDistance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.0128111795041359 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "25" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "08866202(2020): 08866202 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    Family and Type = "08866202(2020): 08866202 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "08866202(2020): 08866202 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    Type Id = "08866202(2020): 08866202 Washbasin faucet, 6 V, Bluetooth" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    NominalDepth = 298.7 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 156.1 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 274.5 (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 286. (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical Engineering(Type) | properties | on 1 type object
    Battery = "Lithium 2CR5 6 V" (IFCTEXT)
    Bluetooth = "4.x" (IFCTEXT)
    Electronic Parts = "Autofocus sensor;Solenoid valve;Low battery indication" (IFCTEXT)
    Operating Voltage = 6. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "08866202(2020)" (IFCTEXT)
    ConvergoRefNr = "0087-2006-0004-FI" (IFCTEXT)
    ManufacturerName = "Hansa" (IFCTEXT)
    ManufacturerURL = "http://www.hansa.com" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "06/07/2020" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Backflow Prevention EN1717 = "AA" (IFCTEXT)
    Customs Code = "84818011" (IFCTEXT)
    EAN Number = "4057304014444" (IFCTEXT)
    EMC Directive = "2014/53/EU" (IFCTEXT)
    EN Standard = "EN 1111 , EN 15091" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Advanced Features = "DZR brass;Waterways without nickel coating;Thermal disinfection according to DVGW W 551;Adjustable settings (via bluetooth)" (IFCTEXT)
    Aerator = "Laminar" (IFCTEXT)
    Afterflow Period = 2120. (IFCREAL)
    Automatic Flush = "off (off/1-120 h)" (IFCTEXT)
    Automatic Flush Period = "30 s (1-1800 s)" (IFCTEXT)
    Connection = "Eccentric unions;;;;" (IFCTEXT)
    Connection Size = "G1/2" (IFCTEXT)
    Flow Rate At 300kPa = 0.00565034667543817 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Wall mounted" (IFCTEXT)
    Installation Width = "CC150± 10 mm" (IFCTEXT)
    Installation and Maintenance = "http://static.hansa.com/manual/08866202" (IFCTEXT)
    Lever Handle = "Temperature control handle" (IFCTEXT)
    Max Flow Period = 211800. (IFCREAL)
    Max. Hot Water Supply = 70.0000000000001 (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = ";Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Protection Class = "IP 55" (IFCTEXT)
    Spare Parts = "http://static.hansa.com/sp/08866202" (IFCTEXT)
    Spout Swivel Range = "120° (60°/0°)" (IFCTEXT)
    Spout Type = "Detachable spout;Swivel spout;;" (IFCTEXT)
    Temperature Adjustments = "THERMO COOL" (IFCTEXT)